{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["DOSSIERS"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":4,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"DOSSIERS","index":0,"n_rows":43,"n_cols":20,"rows_kept":43,"cut":false,"hidden":false,"merged":[[0,15,1,15],[0,10,0,11],[0,8,1,8],[0,13,1,13],[0,14,1,14],[0,0,1,0],[0,12,1,12],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,1,5],[0,9,1,9],[0,7,1,7],[0,6,1,6]]}
["N° d'ordre","Centrale d'enrobage","Localisation","CPD - 2 +","Note Justificative","Type d'enrobé","Utilisation pour","Type de liant","% de recyclé","Dossier","Etude réalisée",null,"Réseau","Valeur du T","Date de notification","Validité de l'étude",{"$f":"EDATE(TODAY(),-12)","v":"2024-05-07"},5,{"$f":"TODAY()","v":"2025-05-07"},3]
[null,null,null,null,null,null,null,null,null,null,"le","par",null,null,null,null,{"$f":"TODAY()","v":"2025-05-07"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"DATE(YEAR(K3)+$R$1,MONTH(K3),DAY(K3))","v":"1904-12-31"}]
[40,"VBA","Haren","1137-CPR-0834/64-65","0834/65/2023/63NE/6034/0","MA-6,3-11","C.60.3 : Couche de protection de l'étanchéité","35/50",null,"VM24/66","2024-11-04","AWV","I","T>6000","2025-04-11","2029-11-04"]
[39,"VBA","Haren","1137-CPR-0834/64-65","0834/65/2023/69NE-6104/0","MA-2-type 1","C.60.1 : couche d'étanchéité","35/50",null,"VM24/65","2024-11-04","AWV","I","T>6000","2025-04-11","2029-11-04"]
[38,"WILLEMEN","Gent","1137-CPD-8243","8243/65/2024/62NB-6504/0","MA-4-1","C.60.5 : Pour réparation de fissures (Pains en asphalte coulé et vrac)","35/50",null,"VM24/63","2024-04-05","MOW","I","T>6000","2025-03-05","2029-04-04"]
[37,"WILLEMEN","Gent","1137-CPD-8243","8243/65/2022/61NE-6109/0","MA-6,3-1","C.60.4 : Pour Revêtement et réparation","35/50",null,"VM22/59","2022-10-28","MOW","III",null,"2024-06-26","2027-10-28"]
[36,"WILLEMEN","Gent","1137-CPD-8243","8243/65/2024/61NE-6205/0","MA-4-1","C.60.4 : Pour Revêtement et réparation","35/50",null,"VM24/26","2024-05-29","CRR","III",null,"2024-06-10","2029-05-29"]
[35,"VBA","Haren","1137-CPR-0834/64-65","834/65/2024/62NE-6204/0","MA-4-9","C.60.2 : Pour élément linéaire","35/50",null,"VM24/21","2024-04-18","MOW","I","T>6000","2024-05-13","2029-04-19"]
[34,"WILLEMEN","Gent","1137-CPD-8243","8243/65/2023/61NE-6008/0","MA-10-1","C.60.4 : Pour Revêtement et réparation","35/50",null,"VM23/50","2023-10-08","MOW","III",null,"2024-05-13","2028-10-09"]
[33,"DECKX","Puurs","1137-CPD-8022","8022/65/2023/62NE-0654/0","MA-10-9","C.60.2 : Pour élément linéaire","35/50",null,"VM23/37","2023-10-23","DECKX","I","T>6000","2023-11-16","2028-10-22"]
[32,"DECKX","Puurs","1137-CPD-8022","8022/65/2023/62NE-0653/0","MA-6,3-9","C.60.2 : Pour élément linéaire","35/50",null,"VM23/34","2023-10-23","DECKX","I","T>6000","2023-11-16","2028-10-22"]
[31,"DECKX","Puurs","1137-CPD-8022","8022/65/2023/62NE-0652/0","MA-4-9","C.60.2 : Pour élément linéaire","35/50",null,"VM23/36","2023-10-23","DECKX","I","T>6000","2023-11-16","2028-10-22"]
[30,"WILLEMEN","Gent","1137-CPD-8243","8243/65/2023/69NE-6306/0","MA 4-type 1","C.60.1 : couche d'étanchéité","35/50",null,"VM23/16","2022-08-10","CRR","I","T>6000","2023-05-16","2027-08-09"]
[29,"WILLEMEN","Gent","1137-CPD-8243","8243/65/2023/63NE-6414/0 ","MA-6,3-11","C.60.3 : Couche de protection de l'étanchéité","35/50",null,"VM23/15","2022-08-10","CRR","I","T>6000","2023-05-16","2027-08-09"]
[28,"DECKX","Puurs","1137-CPD-8022","8022/65/2022/62NE-0649/0","MA-4-9","C.60.4 : Pour Revêtement et réparation","35/50",null,"VM22/52","2023-05-31","MOW","III",null,"2023-06-02","2028-05-31"]
[27,"DECKX","Puurs","1137-CPD-8022","8022/65/2022/62NE-2616/0","MA 2-type 1","C.60.5 : Pour réparation de fissures (Pains en asphalte coulé et vrac)","35/50",null,"VM22/51","2022-03-24","ACAP","I","T>6000","2023-04-28","2027-02-20"]
[26,"DECKX","Puurs","1137-CPD-8022","8022/65/2021/69NE-2614/0 ","MA 2-type 1","C.60.3 : Couche de protection de l'étanchéité","15/25",null,"VM22/50","2022-03-24","ACAP","I","T>6000","2023-04-28","2027-03-23"]
[25,"DECKX","Puurs","1137-CPD-8022","8022/65/2021/63NE-1636/0","MA-6,3-8","C.60.3 : Couche de protection de l'étanchéité","15/25",null,"VM21/34","2022-05-17","MOW","I","T>6000","2022-06-30","2027-06-01"]
[24,"WILLEMEN","Gent","1137-CPD-8243","8243/65/2020/62NE-6504/0","MA-type 1","C.60.5 : Pour réparation de fissures (Pains en asphalte coulé et vrac)","35/50",null,"VM20/69","2020-10-07","AWV","I",null,"2021-01-07","2025-10-06"]
[23,"WILLEMEN","Gent","1137-CPD-8243","8243/65/2020/61NE-6203/0","MA-4-1","C.60.2 : Pour élément linéaire","35/50",null,"VM20/68","2020-10-07","AWV","IIb",null,"2021-01-07","2025-10-06"]
[22,"WILLEMEN","Gent","1137-CPD-8243","8243/65/2020/61NE-6202/0","MA-4-1","C.60.2 : Pour élément linéaire","35/50",null,"VM20/61","2020-10-07","AWV","IIb",null,"2021-01-07","2025-10-06"]
[21,"Gravaubel","Liège","1137-CPD-708/64-65","708/403-413/3","MA-6,3-1","C.60.3 : Couche de protection de l'étanchéité","35/50",null,"VM20/12","2020-03-20","CRR","III",null,"2020-05-15","2025-03-19"]
[20,"Gravaubel","Liège","1137-CPD-708/64-65","708/402-412/3","MA-4-9","C.60.2 : Pour élément linéaire","35/50",null,"VM20/12","2020-03-20","SPW","I","T>6000","2020-05-15","2025-03-19"]
[19,"Gravaubel","Liège","1137-CPD-708/64-65","708/424/3","MA-10-9","C.60.4 : Pour Revêtement et réparation","35/50",null,"VM20/07","2020-03-20","CRR","III",null,"2020-05-15","2025-03-19"]
[18,"VBA","Haren","1137-CPR-0834/64-65","834/65/2018/62NE-6420/0","MA 2-type 1","C.60.5 : Pour réparation de fissures (Pains en asphalte coulé et vrac)","35/50",null,"VM18/15","2018-03-26","VBA","I","T>6000","2018-04-05","2023-03-26"]
[17,"VBA","Haren","1137-CPR-0834/64-65","834/65/2018/62NE-6202/0","MA-4-9","C.60.2 : Pour élément linéaire","35/50",null,"VM18/53","2018-09-04","AWV","I","T>6000","2018-11-19","2023-09-04"]
[16,"WILLEMEN","Gent","1137-CPD-8243","8243/65/2017/63NE-6402/0","MA-6,3-1","C.60.3 : Couche de protection de l'étanchéité","35/50",null,"VM17/84","2018-04-16","AWV","III",null,"2018-09-05","2023-04-16"]
[15,"ASWEBO","Gent","1137-CPD-8243","8243/65/2017/63NE-6400/0","MA-6,3-11","C.60.3 : Couche de protection de l'étanchéité","35/50",null,"VM17/83","2017-09-08","AWV","I","T>6000","2018-07-13","2022-09-08"]
[14,"ASWEBO","Gent","1137-CPD-8243","8243/65/2017/63NE-6404/0","MA-6,3-11","C.60.3 : Couche de protection de l'étanchéité","35/50",null,"VM17/82","2017-09-08","AWV","I","T>6000","2018-07-13","2022-09-08"]
[13,"VBA","Haren","1137-CPR-0834/64-65","834/65/2017/69NE-6101/0","MA 2-type 1","C.60.1 : couche d'étanchéité","20/30",null,"VM17/70","2017-09-27","AWV","I","T>6000","2018-05-09","2022-09-27"]
[12,"VBA","Haren","1137-CPR-0834/64-65","834/65/2017/62NE-6031/0","MA-6,3-11","C.60.3 : Couche de protection de l'étanchéité","20/30",null,"VM17/62","2017-09-27","AWV","I","T>6000","2018-03-16","2022-09-27"]
[11,"Gravaubel","Liège","1137-CPD-708/64-65","708/427/3","MA-6,3-11","C.60.4 : Pour Revêtement et réparation","35/50",null,"VM17/61","2017-09-26","GRAVAUBEL","III",null,"2018-03-07","2022-09-26"]
[10,"DECKX","Grobbendonk","1137-CPD-8021","8021/65/2017/62NE-0618/0","MA-4-9","C.60.2 : Pour élément linéaire","35/50",null,"VM17/60","2017-03-24","MDV","I","T>6000","2018-03-06","2022-03-24"]
[9,"DECKX","Puurs","1137-CPD-8022","8022/65/2017/62NE-0618/0","MA-4-9","C.60.2 : Pour élément linéaire","35/50",null,"VM17/60","2017-03-24","MDV","I","T>6000","2018-03-06","2022-03-24"]
[8,"DECKX","Grobbendonk","1137-CPD-8021","8021/65/2017/62NE-0616/0","MA-2-type1","C.60.5 : Pour réparation de fissures (Pains en asphalte coulé et vrac)","35/50",null,"VM17/59","2017-03-24","MDV","I","T>6000","2018-03-06","2022-03-24"]
[7,"DECKX","Puurs","1137-CPD-8022","8022/65/2017/62NE-0616/0","MA-2-type1","C.60.5 : Pour réparation de fissures (Pains en asphalte coulé et vrac)","35/50",null,"VM17/59","2017-03-24","MDV","I","T>6000","2018-03-06","2022-03-24"]
[6,"DECKX","Grobbendonk","1137-CPD-8021","8021/65/2017/69NE-0614/0","MA-2-type1","C.60.1 : couche d'étanchéité","15/25",null,"VM17/58","2017-06-11","AWV","I","T>6000","2018-03-06","2022-06-11"]
[5,"DECKX","Puurs","1137-CPD-8022","8022/65/2017/69NE-0614/0","MA-2-type1","C.60.1 : couche d'étanchéité","15/25",null,"VM17/58","2017-06-11","AWV","I","T>6000","2018-03-06","2022-06-11"]
[4,"DECKX","Grobbendonk","1137-CPD-8021","8021/65/2017/63NE-0636/0","MA-6,3-11","C.60.3 : Couche de protection de l'étanchéité","35/50",null,"VM17/45","2017-06-18","MOW","I","T>6000","2018-01-19","2022-05-18"]
[3,"DECKX","Puurs","1137-CPD-8022","8022/65/2017/63NE-0636/0","MA-6,3-11","C.60.3 : Couche de protection de l'étanchéité","35/50",null,"VM17/45","2017-06-18","MOW","I","T>6000","2018-01-19","2022-05-18"]
[2,"Gravaubel","Liège","1137-CPD-708/64-65","708/428/3","MA-6,3-11","C.60.4 : Pour Revêtement et réparation","35/50",null,"VM17/32","2017-09-21","GRAVAUBEL","III",null,"2017-10-03","2022-09-21"]
[1,"ASWEBO","Gent","1137-CPD-8243","8243/65/2016/62NE-6104/0","MA-4-11","C.60.2 : Pour élément linéaire","35/50",null,"VM16/65","2016-11-23","CRR","I","T>6000","2016-12-14","2021-11-23"]